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A
40W USB-C Ouput

 
Caution
Please read all warnings for your safety and optimal user experience. Please read and follow these instructions carefully and retain for your records. 
1.	Do not disassemble or throw into fire or water.
2.	Do not expose to extreme weather conditions.
3.	Do not use this product if you observe visible defects.
4.	Do not short circuit the product or store it in a receptacle where it may be short circuited by other metallic or conductive objects.
5	Do not operate the product if it has been wet or otherwise damaged, to prevent against electric shock, explosion and/or injury.
6.	Never attempt to dismantle the unit.
7.	Children should be supervised to ensure that they do not play with the product.
8.	Always disconnect the device when not in use.
9.	Do not use if broken, damaged, or exposed to liquids.
10.	Not to be used in extremely high ambient temperatures.
11.	Do not use with damaged or faulty accessories.
12.	Do not place near any sources of heat, open flame, or liquid.
13.	The wall charger is for indoor use only, the maximum ambient temperature is 25°C.


Installation Instructions
Total power output is the measured in Watts and is the maximum output that the wall charger can safely provide when all the USB ports are in use. This is different from an individual ports maximum output (which is higher than the total power output).
Best for charging devices that accept USB power, including phones and tablets from Apple, Samsung, Google, Sony, as well as power banks, hand-held gaming devices and cameras.
For Use with Cygnett, Apple, Samsung, Google, Sony brand IT/AV equipment.
The Wall Charger is for indoor use only; the maximum ambient temperature is 25oC.
Name
40W USB-C Single Wall Charger
Item Number
CY6211PDWCH
CY6212PDWCH
CY6213PDWCH
CY6214PDWCH
CY6215PDWCH
Input (s)
AC: 200-240V, 50-60Hz, 1.0A Max
Output (s)
5.0V⎓3.0A (15.0W); 9.0V⎓3.0A (27.0W); 12V⎓3.0A (36.0W); 15V⎓2.67A (40.0W); 20V⎓2.0A (40.0W)
PPS: 5.0-21.0V-2.0A
AVS:9.0-20.0V/2.67A, 2.0A
Total Output
40.0W Max
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40W USB-C Single Wall Charger


USER MANUAL
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